
**Interception rods system**



**ZIP file is incluiding the following items:**


The ZIP file contains Revit Family files, project file and guide book:

* OBO\_TBS\_Interception\_Rods\_Systems\_Showcase.rvt
* Folders:
  + 1m-4m\_I\_II\_III\_wind\_zone:
    - I\_wind\_zone
      * OBO\_F-FIX-JUNIOR\_Fangfix\_Junior\_5403308\_1m\_I\_II\_III\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_1.5m\_I\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_2m\_I\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_2.5m\_I\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_3m\_I\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_3.5m\_I\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_4m\_I\_wind\_zone.rfa
    - II\_wind\_zone
      * OBO\_Interception rods\_system\_1.5m\_II\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_2m\_II\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_2.5m\_II\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_3m\_II\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_3.5m\_II\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_4m\_II\_wind\_zone.rfa
    - III\_wind\_zone
      * OBO\_Interception rods\_system\_1.5m\_III\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_2m\_III\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_2.5m\_III\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_3m\_III\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_3.5m\_III\_wind\_zone.rfa
      * OBO\_Interception rods\_system\_4m\_III\_wind\_zone.rfa
  + 4m-8m
    - OBO\_isFang\_Fangmast\_System\_4-8m\_TS0012-16.rfa
  + 10m
    - OBO\_irod10\_Fangmast\_System\_10m\_TS0107.rfa
* Guide book.pdf

**About the BIM models**

* **Family Category:**

Project Browser 🡪 Families 🡪 Special Equipment

* **Options for Loading Family to a Project:**
* Drag and drop the family file into an open project file
* Open the Family file 🡪 Family Editor 🡪 Load into Project (choose the project)
* Open Showcase file 🡪 Open your project file 🡪 Manage 🡪 Transfer Project Standards (copy from: Showcase file) – The loaded families will be under the correct family type


The Showcase file contains a part of the BIM models of Interception rods systems from 1m to 10m.


All the BIM models are face-based and have data of products such as Item Name, Item Number, Weight, Material, etc.

**The Interception rods from 1 to 4m:**

The Interception rods from 1-4m are available in I-II-III wind zones.

You can switch between the loaded families by a drop-down menu under the Properties tab.





Under the construction tab you can find the assigned Type rod.


**The Interception rods from 4 to 8m:**

One family file includes the isFang Fangmast systems from 4m to 8m as Type Families.

You can switch between the loaded families by a drop-down menu under the Properties tab.

Under the construction tab there are 2 parameters that are assigned the appropriate types:

* Air-termination rod Type
* Leg Type



**The ’Interception rod 10m’:**

The Family contains only one family type.

**Making schedules:**

The familiy contains shared parameters which can be listed.

